Timeout

Sendto(sendMsg)

start\_timer

Wait for call 0 from above

Wait for call 1 from above

Wait for ACK 1

Wait for ACK 0

Server

Sendto(data)

packet\_num = ‘0’

sendMsg = read(1024) + packet\_num

sendto(sendMsg)

start\_timer

Sendto(data)

packet\_num = ‘1’

sendMsg = read(1024) + packet\_num

sendto(sendMsg)

start\_timer

recvfrom(1024), ACK == 0

stoptimer